,Wattage Comments##OTHER##,WEIGHT##MASS##KILOGRAMS,WATTAGE##ELECTRICAL_WATTAGE##WATTS,VOLTAGE RANGE V##OTHER##,VOLTAGE COMMENTS##OTHER##,VOLTAGE##ELECTRICAL_POTENTIAL##VOLTS,URL##OTHER##,Type Comments##OTHER##,TECHNICAL SHEET##OTHER##,STRUCTURE MATERIAL##OTHER##,RADIUS##LENGTH##MILLIMETERS,PRODUCT SHEET##OTHER##,PRODUCT CODE##OTHER##,OPTIC_DIAM-70##OTHER##,OPTIC_DIAM-134##OTHER##,Model##OTHER##,Manufacturer##OTHER##,MATERIAL DESCRIPTION##OTHER##,Lamp##OTHER##,LIGHTING SPECIFICATION##OTHER##,LIGHTING MATERIAL##OTHER##,HEIGHT##LENGTH##MILLIMETERS,FREQUENCY RANGE Hz##OTHER##,E04220##OTHER##,E04200##OTHER##,Description##OTHER##,Default Elevation##LENGTH##MILLIMETERS,DIAMETER##LENGTH##MILLIMETERS,COLOR RENDERING INDEX##OTHER##,COLLECTION##OTHER##,BIM USER MANUAL##OTHER##,BIM BADGE##OTHER##,BIM AUTHOR##OTHER##,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,AVAILABLE FINISHES##OTHER##,ASSEMBLY SHEET##OTHER##,ACCESSORY CODE##OTHER##,ACCESSORIES##OTHER##
Ø70_H279_DirectLight_Black_COB-LED_12W_2700K_702lm_45°,,0.900000000000,12.000000000000,220-240V,,0.000000000000,https://www.luceplan.com/,,https://www.luceplan.com/products/e04-ceiling,LUCEPLAN_ALUMINIUM_MATT-BLACK,35.000000000000,https://www.archiproducts.com/en/products/luceplan/led-adjustable-extruded-aluminium-ceiling-lamp-e04-ceiling-lamp_349376,1E0400200001+1E040/1M0000,1,0,E04200+E041M,Luceplan S.r.l.,aluminum extrusion cylindrical body,dimmable push/DALI,LED module COB dimmable push/DALI CRI 90,DEFAULT_LIGHT_MATERIAL,279.000000000000,50/60Hz,0,1,Ceiling lights produced in two diameters (70 mm and 134 mm) and various lengths. The recessed positioning of the light source increases the angle of shading and lighting comfort.,0.000000000000,70.000000000000,90,E04 CEILING,https://img.edilportale.com/bim/LUCEPLAN-BIM-USER-MANUAL-LUCEPLAN-bim.pdf,https://bim.archiproducts.com/en/badge/bim-archiproducts-featured_658700/about,https://bim.archiproducts.com,0.000000000000,"Structure: matt black, matt white, matt alu, matt brass. For further info about finishes and codes, please refer to the TECHNICAL SHEET.",https://www.luceplan.com/assets/E04_ceiling-1573736952.pdf,,
Ø134_H372_DirectLight_Black_COB-LED_19W_2700K_1030lm_45°,,1.850000000000,19.000000000000,220-240V,,0.000000000000,https://www.luceplan.com/,,https://www.luceplan.com/products/e04-ceiling,LUCEPLAN_ALUMINIUM_MATT-BLACK,67.000000000000,https://www.archiproducts.com/en/products/luceplan/led-adjustable-extruded-aluminium-ceiling-lamp-e04-ceiling-lamp_349376,1E0400220001+1E040/2M0000,0,1,E04220+E042M,Luceplan S.r.l.,aluminum extrusion cylindrical body,dimmable push/DALI,LED module COB dimmable push/DALI CRI 90,DEFAULT_LIGHT_MATERIAL,372.000000000000,50/60Hz,1,0,Ceiling lights produced in two diameters (70 mm and 134 mm) and various lengths. The recessed positioning of the light source increases the angle of shading and lighting comfort.,0.000000000000,134.000000000000,90,E04 CEILING,https://img.edilportale.com/bim/LUCEPLAN-BIM-USER-MANUAL-LUCEPLAN-bim.pdf,https://bim.archiproducts.com/en/badge/bim-archiproducts-featured_658700/about,https://bim.archiproducts.com,0.000000000000,"Structure: matt black, matt white, matt alu, matt brass. For further info about finishes and codes, please refer to the TECHNICAL SHEET.",https://www.luceplan.com/assets/E04_ceiling-1573736952.pdf,,
