,Wattage Comments##OTHER##,WEIGHT##MASS##KILOGRAMS,WATTAGE##ELECTRICAL_WATTAGE##WATTS,VOLTAGE RANGE V##OTHER##,VOLTAGE COMMENTS##OTHER##,VOLTAGE##ELECTRICAL_POTENTIAL##VOLTS,URL##OTHER##,Type Comments##OTHER##,TECHNICAL SHEET##OTHER##,STRUCTURE MATERIAL##OTHER##,RADIUS##LENGTH##MILLIMETERS,PRODUCT SHEET##OTHER##,PRODUCT CODE##OTHER##,OPTIC_DIAM-70_UPWARD##OTHER##,OPTIC_DIAM-70_DOWNWARD##OTHER##,OPTIC_DIAM-134_UPWARD##OTHER##,OPTIC_DIAM-134_DOWNWARD##OTHER##,Model##OTHER##,Manufacturer##OTHER##,MATERIAL DESCRIPTION##OTHER##,Lamp##OTHER##,LIGHTING SPECIFICATION##OTHER##,LIGHTING MATERIAL##OTHER##,HEIGHT##LENGTH##MILLIMETERS,FREQUENCY RANGE Hz##OTHER##,Description##OTHER##,Default Elevation##LENGTH##MILLIMETERS,DIAMETER##LENGTH##MILLIMETERS,DIAM70##OTHER##,DIAM134##OTHER##,CORD LENGTH CONTROL##LENGTH##MILLIMETERS,CORD LENGTH##LENGTH##MILLIMETERS,COLOR RENDERING INDEX##OTHER##,COLLECTION##OTHER##,BIM USER MANUAL##OTHER##,BIM BADGE##OTHER##,BIM AUTHOR##OTHER##,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,AVAILABLE FINISHES##OTHER##,ASSEMBLY SHEET##OTHER##,ACCESSORY CODE##OTHER##,ACCESSORIES##OTHER##
Ø70_H279_DirectLight_Black_COB-LED_12W_2700K_702lm_45°,,0.950000000000,12.000000000000,220-240V,,0.000000000000,https://www.luceplan.com/,,https://www.luceplan.com/products/e04-suspension,LUCEPLAN_ALUMINIUM_MATT-BLACK,35.000000000000,https://www.archiproducts.com/en/products/luceplan/led-extruded-aluminium-pendant-lamp-e04-pendant-lamp_349374,1E0400270001+1E040/1M0000+1EA100096000,0,1,0,0,E04270+E041M+EA1096,Luceplan S.r.l.,aluminum extrusion cylindrical body,dimmable push/DALI,LED module COB dimmable push/DALI CRI 90,DEFAULT_LIGHT_MATERIAL,279.000000000000,50/60Hz,"Aluminium suspensions in two diameters and different lengths. The power cable enters the side of the cylinder, providing two-way emission without casting a shadow on the ceiling. The light source in a recessed position, preventing glare and improving visual comfort.",0.000000000000,70.000000000000,1,0,1000.000000000000,1000.000000000000,90,E04 SUSPENSION,https://img.edilportale.com/bim/LUCEPLAN-BIM-USER-MANUAL-LUCEPLAN-bim.pdf,https://bim.archiproducts.com/en/badge/bim-archiproducts-featured_658700/about,https://bim.archiproducts.com,0.000000000000,"Structure: matt black, matt white, matt alu, matt brass. For further info about finishes and codes, please refer to the TECHNICAL SHEET.",https://www.luceplan.com/assets/E04_suspension-1573736985.pdf,,
Ø70_H465_Direct-IndirectLight_Black_COB-LED_12W_2700K_702lm_45°,2x12W,2.000000000000,24.000000000000,220-240V,,0.000000000000,https://www.luceplan.com/,,https://www.luceplan.com/products/e04-suspension,LUCEPLAN_ALUMINIUM_MATT-BLACK,35.000000000000,https://www.archiproducts.com/en/products/luceplan/led-extruded-aluminium-pendant-lamp-e04-pendant-lamp_349374,1E0400280001+1E040/1M0000 (X2)+1EA100096000,1,1,0,0,E04280+E041M(x2)+EA1096,Luceplan S.r.l.,aluminum extrusion cylindrical body,dimmable push/DALI,LED module COB dimmable push/DALI CRI 90,DEFAULT_LIGHT_MATERIAL,465.000000000000,50/60Hz,"Aluminium suspensions in two diameters and different lengths. The power cable enters the side of the cylinder, providing two-way emission without casting a shadow on the ceiling. The light source in a recessed position, preventing glare and improving visual comfort.",0.000000000000,70.000000000000,1,0,1000.000000000000,1000.000000000000,90,E04 SUSPENSION,https://img.edilportale.com/bim/LUCEPLAN-BIM-USER-MANUAL-LUCEPLAN-bim.pdf,https://bim.archiproducts.com/en/badge/bim-archiproducts-featured_658700/about,https://bim.archiproducts.com,0.000000000000,"Structure: matt black, matt white, matt alu, matt brass. For further info about finishes and codes, please refer to the TECHNICAL SHEET.",https://www.luceplan.com/assets/E04_suspension-1573736985.pdf,,
Ø134_H372_DirectLight_Black_COB-LED_19W_2700K_1030lm_45°,,2.300000000000,19.000000000000,220-240V,,0.000000000000,https://www.luceplan.com/,,https://www.luceplan.com/products/e04-suspension,LUCEPLAN_ALUMINIUM_MATT-BLACK,67.000000000000,https://www.archiproducts.com/en/products/luceplan/led-extruded-aluminium-pendant-lamp-e04-pendant-lamp_349374,1E0400290001+1E040/2M0000+1EA100096000,0,0,0,1,E04290+E042M+EA1096,Luceplan S.r.l.,aluminum extrusion cylindrical body,dimmable push/DALI,LED module COB dimmable push/DALI CRI 90,DEFAULT_LIGHT_MATERIAL,372.000000000000,50/60Hz,"Aluminium suspensions in two diameters and different lengths. The power cable enters the side of the cylinder, providing two-way emission without casting a shadow on the ceiling. The light source in a recessed position, preventing glare and improving visual comfort.",0.000000000000,134.000000000000,0,1,1000.000000000000,1000.000000000000,90,E04 SUSPENSION,https://img.edilportale.com/bim/LUCEPLAN-BIM-USER-MANUAL-LUCEPLAN-bim.pdf,https://bim.archiproducts.com/en/badge/bim-archiproducts-featured_658700/about,https://bim.archiproducts.com,0.000000000000,"Structure: matt black, matt white, matt alu, matt brass. For further info about finishes and codes, please refer to the TECHNICAL SHEET.",https://www.luceplan.com/assets/E04_suspension-1573736985.pdf,,
