,WATTAGE##ELECTRICAL_WATTAGE##WATTS,VOLTAGE RANGE##OTHER##,URL##OTHER##,TECHNICAL SHEET##OTHER##,PRODUCT SHEET##OTHER##,PRODUCT CODE##OTHER##,Model##OTHER##,Manufacturer##OTHER##,MATERIAL DESCRIPTION##OTHER##,Lamp##OTHER##,LIGHTING SPECIFICATION##OTHER##,HEIGHT##LENGTH##MILLIMETERS,Description##OTHER##,Default Elevation##LENGTH##MILLIMETERS,DIAMETER##LENGTH##MILLIMETERS,DEPTH##LENGTH##MILLIMETERS,CRI##OTHER##,CORD LENGTH##LENGTH##MILLIMETERS,COLLECTION##OTHER##,BODY MATERIAL##OTHER##,BIM USER MANUAL##OTHER##,BIM BADGE##OTHER##,BIM AUTHOR##OTHER##,AVAILABLE FINISHES##OTHER##
White,19.000000000000,100V - 277V,https://www.estiluz.com/en,,,T-4064,Mood T-4064S,Estiluz,Metal,LED 19W,LED 19W (2700K / Ang.120º / >80 CRI / 24V) 100V - 277V / Typ* 1800 lumens Dimmable 1-10V,600.000000000000,"Metallic suspension lamp providing direct or indirect light. Shade is completely independent of the support magnet and it can be mounted facing up, own or in any position even after installation. Adjustable height. Recessed canopy version requires false ceiling and Ø85mm drill.",1219.200000000000,270.000000000000,270.000000000000,>80,600.000000000000,Mood,ESTILUZ_METAL_74_WH,https://bimcad.edilportale.com/ESTILUZ-BIM-USER-MANUAL-Estiluz-bim.pdf,https://bim.archiproducts.com/en/badge/bim-archiproducts-featured_658700/about,https://bim.archiproducts.com,"White, Nude, CUSTOM"
